初始化：
1）初始化广播搜索回调 NET_CARD_BroadcastSerachDevice(GetBroadcastSerachProcess);
2）初始化实时监控回调 NET_CARD_RealTimeDataCallback(GetRealtimeDataProcess);
3）初始化身份证与二维码回调函数 NET_CARD_RealTimeDataCallbackEx(GetRealtimeDataProcessEx);


1)设置UDP二维码身份证信息上传服务器IP与端口 NET_CARD_Set_QR_ServerUDPIPAndPort
2)设置UDP所有记录上传服务器IP与端口 NET_CARD_Set_RecordUpLoad_UDPIPAndPort
3)开启实时监控 NET_CARD_EnableRealTimeMonitor

  开启实时监控，刷卡记录信息才能上来，但不开实时监控二维码与身份证信息的上传也能上传



INIT STEP：
1）Set Broadcast CallBack Function
   NET_CARD_BroadcastSerachDevice(GetBroadcastSerachProcess);
2）Set RealTime CallBack Function
   NET_CARD_RealTimeDataCallback(GetRealtimeDataProcess);
3）Set IDcard OR QR Code CallBack Function
   NET_CARD_RealTimeDataCallbackEx(GetRealtimeDataProcessEx);

INIT UDP Server IP and Port
1)Set QR Recieve Server IP and Port 
  NET_CARD_Set_QR_ServerUDPIPAndPort
2)Set Record Event Recieve Server IP and Port
  NET_CARD_Set_RecordUpLoad_UDPIPAndPort
3)Start RealTime monitor
  NET_CARD_EnableRealTimeMonitor
  Must call the "Start RealTime monitor",and the "Record Event" will be sent to "Record Event Recieve Server IP and Port"






